Features Configuration Bits RAM map SFR map

PIC18LF24J11
CONFIG1L (address:0x003FF8, mask:0xE1, default:0xE1)
WDTEN -- Watchdog Timer (bitmask:0x01)
WDTEN = OFF | 0x00 | Disabled - Controlled by SWDTEN bit.
WDTEN = ON | 0x01 | Enabled.
STVREN -- Stack Overflow/Underflow Reset (bitmask:0x20)
STVREN = OFF | 0x00 | Disabled.
STVREN = ON | 0x20 | Enabled.
XINST -- Extended Instruction Set (bitmask:0x40)
XINST = OFF | 0x00 | Disabled.
XINST = ON | 0x40 | Enabled.
DEBUG -- Background Debug (bitmask:0x80)
DEBUG = ON | 0x00 | Enabled.
DEBUG = OFF | 0x80 | Disabled.
CONFIG1H (address:0x003FF9, mask:0x04, default:0x04)
CP0 -- Code Protect (bitmask:0x04)
CP0 = ON | 0x00 | Program memory is code-protected.
CP0 = OFF | 0x04 | Program memory is not code-protected.
CONFIG2L (address:0x003FFA, mask:0xDF, default:0xDF)
OSC -- Oscillator (bitmask:0x07)
OSC = INTOSC | 0x00 | INTOSC.
OSC = INTOSCO | 0x01 | INTOSCO (CLKO-RA6).
OSC = INTOSCPLL | 0x02 | INTOSCPLL.
OSC = INTOSCPLLO | 0x03 | INTOSCPLLO (CLKO-RA6).
OSC = HS | 0x04 | HS.
OSC = HSPLL | 0x05 | HS+PLL.
OSC = EC | 0x06 | EC (CLKO-RA6).
OSC = ECPLL | 0x07 | EC+PLL (CLKO-RA6).
T1DIG -- T1OSCEN Enforcement (bitmask:0x08)
T1DIG = OFF | 0x00 | Secondary Oscillator clock source may not be selected.
T1DIG = ON | 0x08 | Secondary Oscillator clock source may be selected.
LPT1OSC -- Low-Power Timer1 Oscillator (bitmask:0x10)
LPT1OSC = ON | 0x00 | Low-power operation.
LPT1OSC = OFF | 0x10 | High-power operation.
FCMEN -- Fail-Safe Clock Monitor (bitmask:0x40)
FCMEN = OFF | 0x00 | Disabled.
FCMEN = ON | 0x40 | Enabled.
IESO -- Internal External Oscillator Switch Over Mode (bitmask:0x80)
IESO = OFF | 0x00 | Disabled.
IESO = ON | 0x80 | Enabled.
CONFIG2H (address:0x003FFB, mask:0x0F, default:0x0F)
WDTPS -- Watchdog Postscaler (bitmask:0x0F)
WDTPS = 1 | 0x00 | 1:1.
WDTPS = 2 | 0x01 | 1:2.
WDTPS = 4 | 0x02 | 1:4.
WDTPS = 8 | 0x03 | 1:8.
WDTPS = 16 | 0x04 | 1:16.
WDTPS = 32 | 0x05 | 1:32.
WDTPS = 64 | 0x06 | 1:64.
WDTPS = 128 | 0x07 | 1:128.
WDTPS = 256 | 0x08 | 1:256.
WDTPS = 512 | 0x09 | 1:512.
WDTPS = 1024 | 0x0A | 1:1024.
WDTPS = 2048 | 0x0B | 1:2048.
WDTPS = 4096 | 0x0C | 1:4096.
WDTPS = 8192 | 0x0D | 1:8192.
WDTPS = 16384 | 0x0E | 1:16384.
WDTPS = 32768 | 0x0F | 1:32768.
CONFIG3L (address:0x003FFC, mask:0xFF, default:0xFF)
DSWDTOSC -- DSWDT Clock Select (bitmask:0x01)
DSWDTOSC = T1OSCREF | 0x00 | DSWDT uses T1OSC/T1CKI.
DSWDTOSC = INTOSCREF | 0x01 | DSWDT uses INTRC.
RTCOSC -- RTCC Clock Select (bitmask:0x02)
RTCOSC = INTOSCREF | 0x00 | RTCC uses INTRC.
RTCOSC = T1OSCREF | 0x02 | RTCC uses T1OSC/T1CKI.
DSBOREN -- Deep Sleep BOR (bitmask:0x04)
DSBOREN = OFF | 0x00 | Disabled.
DSBOREN = ON | 0x04 | Enabled.
DSWDTEN -- Deep Sleep Watchdog Timer (bitmask:0x08)
DSWDTEN = OFF | 0x00 | Disabled.
DSWDTEN = ON | 0x08 | Enabled.
DSWDTPS -- Deep Sleep Watchdog Postscaler (bitmask:0xF0)
DSWDTPS = 2 | 0x00 | 1:2 (2.1 ms).
DSWDTPS = 8 | 0x10 | 1:8 (8.3 ms).
DSWDTPS = 32 | 0x20 | 1:32 (33 ms).
DSWDTPS = 128 | 0x30 | 1:128 (132 ms).
DSWDTPS = 512 | 0x40 | 1:512 (528 ms).
DSWDTPS = 2048 | 0x50 | 1:2,048 (2.1 seconds).
DSWDTPS = 8192 | 0x60 | 1:8,192 (8.5 seconds).
DSWDTPS = K32 | 0x70 | 1:32,768 (34 seconds).
DSWDTPS = K131 | 0x80 | 1:131,072 (135 seconds).
DSWDTPS = K524 | 0x90 | 1:524,288 (9 minutes).
DSWDTPS = M2 | 0xA0 | 1:2,097,152 (36 minutes).
DSWDTPS = M8 | 0xB0 | 1:8,388,608 (2.4 hours).
DSWDTPS = M33 | 0xC0 | 1:33,554,432 (9.6 hours).
DSWDTPS = M134 | 0xD0 | 1:134,217,728 (38.5 hours).
DSWDTPS = M536 | 0xE0 | 1:536,870,912 (6.4 days).
DSWDTPS = G2 | 0xF0 | 1:2,147,483,648 (25.7 days).
CONFIG3H (address:0x003FFD, mask:0x09, default:0x09)
IOL1WAY -- IOLOCK One-Way Set Enable bit (bitmask:0x01)
IOL1WAY = OFF | 0x00 | The IOLOCK bit (PPSCON<0>) can be set and cleared as needed.
IOL1WAY = ON | 0x01 | The IOLOCK bit (PPSCON<0>) can be set once.
MSSP7B_EN -- MSSP address masking (bitmask:0x08)
MSSP7B_EN = MSK5 | 0x00 | 5 Bit address masking mode.
MSSP7B_EN = MSK7 | 0x08 | 7 Bit address masking mode.
CONFIG4L (address:0x003FFE, mask:0xCF, default:0xCF)
WPFP -- Write/Erase Protect Page Start/End Location (bitmask:0x0F)
WPFP = PAGE_0 | 0x00 | Write Protect Program Flash Page 0.
WPFP = PAGE_1 | 0x01 | Write Protect Program Flash Page 1.
WPFP = PAGE_2 | 0x02 | Write Protect Program Flash Page 2.
WPFP = PAGE_3 | 0x03 | Write Protect Program Flash Page 3.
WPFP = PAGE_4 | 0x04 | Write Protect Program Flash Page 4.
WPFP = PAGE_5 | 0x05 | Write Protect Program Flash Page 5.
WPFP = PAGE_6 | 0x06 | Write Protect Program Flash Page 6.
WPFP = PAGE_7 | 0x07 | Write Protect Program Flash Page 7.
WPFP = PAGE_8 | 0x08 | Write Protect Program Flash Page 8.
WPFP = PAGE_9 | 0x09 | Write Protect Program Flash Page 9.
WPFP = PAGE_10 | 0x0A | Write Protect Program Flash Page 10.
WPFP = PAGE_11 | 0x0B | Write Protect Program Flash Page 11.
WPFP = PAGE_12 | 0x0C | Write Protect Program Flash Page 12.
WPFP = PAGE_13 | 0x0D | Write Protect Program Flash Page 13.
WPFP = PAGE_14 | 0x0E | Write Protect Program Flash Page 14.
WPFP = PAGE_15 | 0x0F | Write Protect Program Flash Page 15.
WPEND -- Write/Erase Protect Region Select (valid when WPDIS = 0) (bitmask:0x40)
WPEND = PAGE_0 | 0x00 | Page 0 through WPFP<5:0> erase/write protected.
WPEND = PAGE_WPFP | 0x40 | Page WPFP<5:0> through Configuration Words erase/write protected.
WPCFG -- Write/Erase Protect Configuration Region (bitmask:0x80)
WPCFG = ON | 0x00 | Configuration Words page erase/write-protected.
WPCFG = OFF | 0x80 | Configuration Words page not erase/write-protected.
CONFIG4H (address:0x003FFF, mask:0x01, default:0x01)
WPDIS -- Write Protect Disable bit (bitmask:0x01)
WPDIS = ON | 0x00 | WPFP<5:0>/WPEND region erase/write protected.
WPDIS = OFF | 0x01 | WPFP<5:0>/WPEND region ignored.

This page generated automatically by the device-help.pl program (2016-08-21 09:07:43 UTC) from the 8bit_device.info file (rev: 1.31) of mpasmx and from the gputils source package (rev: svn Unversioned directory). The mpasmx is included in the MPLAB X.