Features Configuration Bits RAM map SFR map

PIC16F570
Coff ID of device | 0xF570
Number of ROM/FLASH pages | 4 (512 words/pages)
Last address of ROM/FLASH | 0x07FF
Size of ROM | 2048 words
Address space of FLASH Data | 0x0800 - 0x083F (64 words)
Address space of User ID | 0x0840 - 0x0843 (4 bytes)
Address of Configuration Word | 0x0FFF (1 word)
Number of RAM Banks | 8 (32 bytes/banks)
Number of SFRs | 25
Size of shared GPRs | 4 bytes
Size of all GPRs | 132 bytes
Joint size of SFRs + GPRs | 157 bytes
Standard header | p16f570.inc
Standard linker script | 16f570_g.lkr

This page generated automatically by the device-help.pl program (2016-08-21 09:07:38 UTC) from the 8bit_device.info file (rev: 1.31) of mpasmx and from the gputils source package (rev: svn Unversioned directory). The mpasmx is included in the MPLAB X.